**GRoVe2 WiFi remote**

The remote uses a 2-axes joystick and an ESP32

|  |  |
| --- | --- |
| **Joystick BOB pin** | **ESP32 pin** |
| GND | GND |
| VCC | 3.3V |
| VRX | GPIO36(A0) |
| VRY | GPIO39(A3) |